For 1990-2009 cars

### Removal Procedure

1. Remove the following subassemblies:

• | The right exhaust manifold--Refer to Exhaust Manifold Replacement - Right Side .

• | The water crossover--Refer to Water Outlet Housing Replacement .

• | The intake manifold--Refer to Intake Manifold Replacement .

• | The right secondary camshaft drive chain--Refer to Secondary Camshaft Drive Chain Replacement - Right Side .

• | The right camshaft--Refer to Camshaft Replacement - Right Side .

2. Remove the right cylinder head. Make sure that no dowel guide pins are stuck in the cylinder head. Refer to Cylinder Head Removal - Right Side .
3. Disassemble the right cylinder head. Refer to Cylinder Head Disassemble .
4. Clean and inspect the cylinder head. Refer to Cylinder Head Cleaning and Inspection .
5. Assemble the right cylinder head. Refer to Cylinder Head Assemble .

### Installation Procedure

1. Install the right cylinder head. Refer to Cylinder Head Installation - Right Side .
2. Install the following subassemblies:

• | The right camshaft--Refer to Camshaft Replacement - Right Side .

• | The right secondary camshaft drive chain--Refer to Secondary Camshaft Drive Chain Replacement - Right Side .

• | The intake manifold--Refer to Intake Manifold Replacement .

• | The water crossover--Refer to Water Outlet Housing Replacement .

• | The right exhaust manifold--Refer to Exhaust Manifold Replacement - Right Side .