For 1990-2009 cars

# Driver Information and Entertainment

## All Description and Operation

- Audible Warnings Description and Operation
- Compass Calibration and Magnetic Variance
- Driver Information Center (DIC) Description and Operation
- Indicator/Warning Message Description and Operation
- Instrument Cluster Description and Operation

## All Special Tools and Equipment

- Special Tools

## Diagnostic Procedures

- Chime Always On
- Chime Inoperative
- Diagnostic Starting Point - Displays and Gages
- Driver Information Center (DIC) Switch Inoperative
- Engine Oil Pressure Indicator Always On
- Engine Oil Temperature Indicator Always On
- Fuel Gage Inaccurate or Inoperative
- Instrument Cluster Gages Inoperative
- Low Engine Oil Level Indicator Always On
- Low Engine Oil Level Indicator Inoperative
- Mirror Compass Display Inoperative or Inaccurate
- MPH (Km/h) Indicator Inoperative
- Symptoms - Displays and Gages
- Tachometer Inaccurate or Inoperative

## Diagnostic Trouble Codes

- DTC B3567
- DTC C0126
- DTC P0461
- DTC P0462
- DTC P0463
- DTC P0464
- DTC P0521
- DTC P0522
- DTC P0523
- DTC P0608
- DTC P2066
- DTC P2067
- DTC P2068

## Electrical/Electronic Schematic Diagrams

- Audible Warnings Schematics
- Instrument Cluster Schematics

## Electrical/Electronic Specifications

- Fuel Level Specifications

## General Diagnostic Information

- Scan Tool Data Definitions
- Scan Tool Data List
- Scan Tool Output Controls

## Mechanical Specifications

- Fastener Tightening Specifications

## Removal, Installation, and Replacement

- Clock Replacement
- Driver Information Display Switch Replacement
- Instrument Cluster Replacement