For 1990-2009 cars

### Removal Procedure

1. Remove the right sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.
2. Disconnect the blower motor control module electrical connectors.
3. Remove the blower motor control module retaining screws.
4. Remove the blower motor control module from the vehicle.

### Installation Procedure

1. Install blower motor control module.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the blower motor control module retaining screws.

Tighten
Tighten the bolt to 1 N·m (9 lb in).

3. connect the electrical connectors to blower motor control module.
4. Install the right sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.