For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Manual Shaft Detent Assembly Caution: Ensure the manual shaft detent assembly roller is centered over the manual shaft detent lever assembly. Failure to center the roller may cause hard or no shift lever operation.
2 | Bolt M6 x 14.5 Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)
3 | NEW Fluid Filter Seal Assembly

#### Special Tools

• | DT 47848 Seal Installer

• | J 42183 Driver Handle

4 | NEW Fluid Filter Assembly