For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the right engine mount bracket. Refer to Engine Mount Bracket Replacement - Right Side.
3. Remove the engine mount retaining nut.
4. Remove the engine mount from the vehicle.

### Installation Procedure

1. Install the engine mount to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

3. Install the right engine mount bracket. Refer to Engine Mount Bracket Replacement - Right Side.
4. Lower the vehicle.