For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Bumper Fascia Assembly Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the air deflector. Refer to Front Air Deflector Replacement.

1 | Front Hood Retainer (Qty: 2)
2 | Front Hood Assembly
3 | Front Hood Retainer (Qty: 2)
4 | Right Front Hood Assembly
5 | Front Hood Retainer (Qty: 2)
6 | Left Front Hood Assembly
7 | Front Bumper Fascia Extension Retainer (Qty: 22)
8 | Front Bumper Fascia Retainer (Qty: 2)
9 | Front Bumper Fascia Side Lamp Electrical Connector Tip Disconnect the front bumper fascia side and fog lamp electrical connector.
10 | Front Bumper Fascia Reinforcement Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
11 | Front Bumper Fascia Reinforcement Screw (Qty: 2) Tighten 9 N·m (80 lb in)
12 | Front Bumper Fascia Assembly (Qty: 4) Tip

1. Remove the retainers holding the fascia to the tie bar
2. If headlamp washer hose assembly is installed, disconnect it.