For 1990-2009 cars

### Removal Procedure

Warning: Do NOT attempt to repair or alter the bracket on the child seat restraint system. If the bracket is damaged, replace the entire bracket. Altering the bracket could result in personal injury.

1. Remove the rear trim shelf panel. Refer to Rear Window Shelf Trim Panel Replacement.
2. Remove the bolt that retains the child tether anchor that is being serviced.
3. Remove the child tether anchor from the vehicle.

### Installation Procedure

Note: During installation, ensure that the child tether anchors are installed with the anti-rotation tabs firmly seated in the anti-rotation tab holes on the cross bar beam.

1. Install the child tether anchor to the cross car beam.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the child tether anchor bolt.

Tighten
Tighten the bolt to 40 N·m (29 lb ft).

3. Install the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.