For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement.
2. Remove the bolts securing the rear of cupholder to the front floor console extension trim panel.
3. Remove the cupholder from the front floor console.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front floor console cupholder.

Tighten
Tighten the screws to 2 N·m (18 lb in).

2. Install the bolts securing the cupholder to the front floor console extension trim panel.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement.