For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bumper Nuts | 25 N·m | 18 lb ft
Catalytic Converter-to-Exhaust Manifold Nuts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Cylinder Head Bolts (LH2) | 25 N·m | 18 lb ft
Exhaust Manifold-to-Cylinder Head Bolts (LY7) | 20 N·m | 15 lb ft
Exhaust Manifold-to-Cylinder Head Nuts (LH2) | 30 N·m | 22 lb ft
Exhaust Manifold-to-Cylinder Head Studs (LH2) | 6 N·m | 53 lb in
Muffler Exhaust Pipe-to-Exhaust Manifold Nuts (LH2) | 30 N·m | 22 lb ft
Muffler Nuts (LY7) | 22 N·m | 16 lb ft
Tunnel Brace Bolts | 25 N·m | 18 lb ft