For 1990-2009 cars

## Door Lock and Side Window Switch Replacement - Driver Side Outlook only with RPO AXA

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove driver side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side .

1 | Front Side Door Lock and Side Window Switch Assembly

#### Procedure

1. Disconnect the electrical connector from the switch assembly.
2. Depress the retainers from the back side of the door panel.
3. Lift upward at the rear edge of the switch assembly then slide up and out of the door panel.

## Door Lock and Side Window Switch Replacement - Driver Side with RPO AXE or AXC

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the driver side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side.

1 | Front Side Door Lock and Side Window Switch Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Front Side Door Lock and Side Window Switch Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Refer to Control Module References for programming and set-up information.

## Door Lock and Side Window Switch Replacement - Driver Side Traverse with RPO AXE

Callout | Component Name
--- | ---
1 | Front Side Door Lock and Side Window Switch Assembly

#### Procedure

1. Lift upward at the rear edge of the switch assembly then slide up and out of the door panel.
2. Disconnect the electrical connector from the switch assembly.