For 1990-2009 cars

## Front Side Door Molding Replacement Acadia

Callout | Component Name
--- | ---
1 | Front Side Door Center Molding Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Using a J 25070 Heat Gun in a circular motion in order to warm and help to remove the front side door molding.
2. Peel the adhesive tape liner from the molding.
3. Align the 3 plastic retainers to the holes in the door.
4. Secure the retainers to the door.
5. Using a clean towel and hand pressure, wet out the entire length of the molding starting at the front edge of the rear door and working rearward.

2 | Front Side Door Center Molding Retainer (Qty: 3)

## Front Side Door Molding Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Front Side Door Center Molding Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 Heat Gun to remove the front side door molding.
2. Peel the adhesive tape liner from the molding.

2 | Front Side Door Retainer (Qty: 3)

#### Procedure

1. Align the 3 retainer clips to the holes in the door.
2. Align the A-pillar clip first followed by the other 2 clips.
3. Push up slightly on the molding when aligning the other 2 holes.
4. Using a clean towel and hand pressure, wet out the entire length of the molding starting at the front edge of the front door and working rearward.