For 1990-2009 cars

## Backup Lamp Bulb Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Back Up Lamp Socket

#### Procedure

Rotate and remove the socket from the lamp assembly.

2 | Back Up Lamp Bulb Tip Remove the bulb and discard.

## Backup Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Back Up Lamp Socket

#### Procedure

Rotate and remove the socket from the lamp assembly.

2 | Back Up Lamp Bulb Tip Remove the bulb and discard.
3 | Marker Lamp Socket
4 | Marker Lamp Bulb

## Backup Lamp Bulb Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Back Up Lamp Socket

#### Procedure

Rotate and remove the socket from the lamp assembly.

2 | Back Up Lamp Bulb Tip Remove the bulb and discard.

## Backup Lamp Bulb Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Back Up Lamp Socket

#### Procedure

1. Disconnect the back up lamp bulb socket electrical connector.
2. Rotate and remove the socket from the back up lamp applique assembly.

2 | Back Up Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Pull the bulb from the lamp socket and discard.