For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the seat belt anchor bolt. Refer to Seat Belt Retractor Replacement - No. 1 Rear .
2. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .

1 | Body Lock Upper Trim Panel Retainer (Qty: 3)
2 | Body Lock Upper Trim Panel Clip
3 | Body Lock Upper Trim Panel Assembly Tip Route the seat belt through the trim panel.