For 1990-2009 cars

## Rear Side Door Molding Replacement Acadia

Callout | Component Name
--- | ---
1 | Rear Side Door Center Molding Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 Heat Gun in a circular motion in order to warm and help to remove the rear side door molding.
2. Peel the adhesive tape liner from the molding.
3. Align the 3 plastic clips to the holes in the door.
4. Align the B pillar clip first followed by the other two clips.
5. Secure the clips using the mandatory sequence as noted.
6. Push up slightly on the molding when aligning the other 2 holes.
7. Using a clean towel and hand pressure, wet out the entire length of the molding starting at the front edge of the rear door and working rearward.

## Rear Side Door Molding Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Rear Side Door Center Molding Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 to remove the rear side door molding.
2. Peel the adhesive tape liner from the molding.
3. Align the 3 metal clips to the holes in the door.
4. Align the B pillar clip first followed by the other 2 clips.
5. Secure the clips using the mandatory sequence as noted.
6. Push up slightly on the molding when aligning the other 2 holes.
7. Using a clean towel and hand pressure, wet out the entire length of the molding starting at the front edge of the rear door and working rearward.