For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the Air Cleaner Outlet Duct. Refer to Air Cleaner Outlet Duct Replacement.

1 | Transmission Fluid Cooler Outlet Hose/Pipe Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Transmission Fluid Cooler Outlet Hose/Pipe Clamp Nut Tighten 22 N·m (16 lb ft)
3 | Transmission Fluid Cooler Outlet Hose/Pipe

#### Procedure

1. Remove the transmission line from the clips securing the line to the transmission and fan shroud.
2. Inspect the transmission fluid level. Refer to Transmission Fluid Check.