For 1990-2009 cars

## Parking and Turn Signal Lamp Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front park, turn and fog lamp assembly bracket. Refer to Parking and Turn Signal Lamp Bracket Replacement.

1 | Front Turn Signal Lamp Assembly Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9.0 N·m (80 lb in)
2 | Front Turn Signal Lamp Assembly Tip Transfer the park turn bulbs as needed.
3 | Front Turn Signal Lamp Assembly Bracket

#### Procedure

Check and adjust the fog lamp aim after the turn signal lamp bracket assembly has been re-installed. Refer to Fog Lamp Aiming.

## Parking and Turn Signal Lamp Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Park and Turn Signal Lamp Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Park and Turn Signal Lamp Assembly

#### Procedure

1. Disconnect the jumper harness from the forward lamp harness connector.
2. Transfer the jumper harness with bulb sockets and bulbs as needed.
3. Remove the lamp assembly from the upper fascia reinforcement bracket.