For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Control Valve Body Bolt M6 x 65 (Qty: 5)
2 | Control Valve Body Bolt M6 x 35 (Qty: 3)
3 | Control Valve Channel Upper Plate Assembly Tip Inspect the upper channel plate bolt pass through holes for damage or burnelling. Any damage near the PCS feed hole could cause leaking around the PCS switch seal. Replace as necessary.
4 | Control Valve Body Bolt M6 x 55 (Qty: 2)
5 | Control Valve Body Bolt M6 x 55 (Qty: 1)
6 | Control Valve Channel Plate Assembly
7 | Control Valve Body Ball Check Valve (Qty: 9)
8 | Control Valve Upper Body Assembly
9 | Control Valve Lower Body Spacer Plate Assembly Tip Discard the spacer plate assembly.
10 | Control Valve Lower Body Assembly