For 1990-2009 cars

## Rear Side Door Lower Molding Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Using a J 25070 Heat Gun in a circular motion, warm the front side door molding prior to removal. Carefully clean the body panel thoroughly prior to bonding the new lower body side molding to the door.

1 | Rear Side Door Lower Molding Locating Pin

#### Procedure

Align the pin to the center of the door prior to securing the retainers.

2 | Lower Molding Integral Retainers (Qty: 10)
3 | Rear Side Lower Door Molding

#### Procedure

Secure the molding to the door and remove the protective liner on the backside of the molding after all of the retainers are secure.

## Rear Side Door Lower Molding Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Using a J 25070 Heat Gun in a circular motion, warm the rear side door molding prior to removal. Carefully clean the body panel thoroughly prior to bonding the new lower body side molding to the door.

1 | Rear Side Door Lower Molding Locating Hole

#### Procedure

Align the pin to the center of the door prior to securing the retainers.

2 | Lower Molding Integral Retainers (Qty: 11)
3 | Rear Side Lower Door Molding

#### Procedure

1. Secure the molding retainers to the door and remove the protective liner on the backside of the molding after all of the retainers are secure.
2. Using a clean shop towel and the palm of the hand, wet out the entire periphery of the molding in order to assure complete adhesion of the lower door bodyside molding.

## Rear Side Door Lower Molding Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Using a J 25070 Heat Gun in a circular motion, warm the front side door molding prior to removal. Carefully clean the body panel thoroughly prior to bonding the new lower body side molding to the door.

1 | Rear Side Door Lower Molding Locating Pin

#### Procedure

Align the pin to the center of the door prior to securing the retainers.

2 | Lower Molding Integral Retainer (Qty: 10)
3 | Rear Side Lower Door Molding

#### Procedure

Secure the molding to the door and remove the protective liner on the backside of the molding after all of the retainers are secure.

## Rear Side Door Lower Molding Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Using a J 25070 Heat Gun in a circular motion, warm the front side of the lower rear door molding prior to removal. Carefully clean the body panel thoroughly prior to bonding the new lower body side molding to the door.

1 | Lower Molding Base Clip Retainers (Qty: 10)

#### Procedure

Use a suitable trim removal tool to disengage the base clip retainers from the door panel.

2 | Rear Side Lower Door Molding Assembly

#### Procedure

1. Close the door prior to engaging the base clip retainers.
2. Peel the adhesive tape backing from the molding.
3. Align the center retainer to the center hole in the door panel.
4. Align the remaining retainers to the adjacent holes.
5. Firmly press the molding into the door beginning at the center base clip retainer and working outward in both directions.