For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side.
2. Remove the sunshade anchor. Refer to Sunshade Anchor Replacement.

1 | Sunshade Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (25 lb in)
2 | Sunshade Assembly

#### Procedure

1. Lower the front of the headliner enough to gain access to the sunshade electrical connector which is glued to the headliner.
2. Disconnect the sunshade electrical connector.