For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Support the engine. Refer to Engine Support Fixture.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Upper Engine Mount Nut Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove and discard the engine mount nut.
2. Disconnect the active engine mount vacuum line, if equipped.
3. Apply threadlocker to the engine mount threads. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Tip
The engine mount nuts must be replaced once removed. Allow adhesive on new engine mounts nuts to cure for 24 hours after replacement.

Tighten
75 N·m (55 lb ft)

2 | Rear Upper Engine Mount Nut

#### Procedure

1. Remove and discard the engine mount nut.
2. Apply threadlocker to the engine mount threads. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Tip
The engine mount nuts must be replaced once removed. Allow adhesive on new engine mounts nuts to cure for 24 hours after replacement.

Tighten
75 N·m (55 lb ft)

3 | Rear Lower Engine Mount Nut

#### Procedure

1. Remove and discard the engine mount nut.
2. Apply threadlocker to the engine mount threads. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Tip
The engine mount nuts must be replaced once removed. Allow adhesive on new engine mounts nuts to cure for 24 hours after replacement.

Tighten
75 N·m (55 lb ft)

4 | Engine Mount Tip To remove the engine mount, use the engine support fixture to raise engine.