For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering column upper trim cover. Refer to Steering Column Upper Trim Cover Replacement .
2. Remove the steering column lower trim cover. Refer to Steering Column Lower Trim Cover Replacement .

1 | Turn Signal Multifunction Switch

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Release the plastic retaining tabs.