For 1990-2009 cars

### Removal Procedure

Caution: Secure the steering wheel utilizing a strap to prevent rotation. Locking of the steering column will prevent damage and a possible malfunction of the SIR system. The steering wheel must be secured in position before disconnecting the following components:

• | The steering column

• | The intermediate shaft

• | The steering gear

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.
1. Turn the steering wheel to the straight forward position and lock it in place.
2. Hoist the vehicle and raise it. Refer to Lifting and Jacking the Vehicle.
3. Disengage the intermediate steering shaft boot from the steering gear and the intermediate steering shaft upper seal.
4. Remove the intermediate steering shaft bolt (1) and separate the intermediate steering shaft from the steering gear.
5. Remove the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
6. Remove the intermediate steering shaft bolt (1) at the steering column, separate the intermediate steering shaft (2), and pull the intermediate steering shaft upper seal (3) from its place.

Note: Spreading both ends of the new or removed intermediate steering shaft while out of the vehicle will help with the installation.

7. Remove the intermediate steering shaft from inside the vehicle.

### Installation Procedure

1. Install the intermediate steering shaft from inside the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the intermediate steering shaft (2) to the steering column, install the intermediate steering shaft bolt (1), and tighten to 22 N·m (16 lb ft).
3. Position the intermediate steering shaft upper seal (3) back in place.
4. Install the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
5. Position the intermediate steering shaft to the steering gear, install the intermediate steering shaft bolt (1), and tighten to 22 N·m (16 lb ft).

Note: Do not tear the intermediate steering shaft boot and install it the in the exact position it came out.

6. Install the intermediate steering shaft boot to the steering gear and the intermediate steering shaft upper seal.