For 1990-2009 cars

### Removal Procedure

1. Remove the engine front cover. Refer to Engine Front Cover Replacement.
2. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement.
3. Remove the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Removal - Right Side.
4. Remove the right bank secondary camshaft drive chain shoe. Refer to Secondary Camshaft Drive Chain Shoe Removal - Right Side.
5. Remove the right bank secondary camshaft drive chain guide. Refer to Secondary Camshaft Drive Chain Guide Removal - Right Side.
6. Remove the right bank secondary camshaft drive chain. Refer to Secondary Camshaft Drive Chain Removal - Right Side.

### Installation Procedure

1. Ensure the stage 1 camshaft timing is correct. Refer to Setting Camshaft Timing.
2. Install the right bank secondary camshaft drive chain. Refer to Secondary Camshaft Drive Chain Installation - Right Side.
3. Install the right bank secondary camshaft drive chain guide. Refer to Secondary Camshaft Drive Chain Guide Installation - Right Side.
4. Install the right bank secondary camshaft drive chain shoe. Refer to Secondary Camshaft Drive Chain Shoe Installation - Right Side.
5. Install the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Installation - Right Side.
6. Install the spark plugs. Refer to Spark Plug Replacement.
7. Install the engine front cover. Refer to Engine Front Cover Replacement.