For 1990-2009 cars

## Front Side Door Trim Panel Replacement - Left Side Traverse

Callout | Component Name
--- | ---
1 | Front Side Door Pull Handle Cover
2 | Front Side Door Inside Handle Bezel Finish Cover
3 | Front Side Door Trim Panel Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Front Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

5 | Front Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the nine retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

6 | Front Side Door Trim Panel Retainer (Qty: 9)

## Front Side Door Trim Panel Replacement - Left Side Acadia

Callout | Component Name
--- | ---
1 | Front Side Door Pull Handle Cover
2 | Front Side Door Inside Handle Bezel Finish Cover
3 | Front Side Door Trim Panel Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Front Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

5 | Front Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

6 | Front Side Door Trim Panel Retainer (Qty: 9)

## Front Side Door Trim Panel Replacement - Left Side Enclave

Callout | Component Name
--- | ---
1 | Front Side Door Pull Handle Cover
2 | Front Side Door Inside Handle Bezel Finish Cover
3 | Front Side Door Trim Panel Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Front Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

5 | Front Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

6 | Front Side Door Trim Panel Retainer (Qty: 9)

## Front Side Door Trim Panel Replacement - Left Side OUTLOOK

Callout | Component Name
--- | ---
1 | Front Side Door Upper Trim Panel Tip Use a plastic trim tool or equivalent to aid in the removal of the trim panel.
2 | Front Side Door Pull Handle Cover
3 | Front Side Door Inside Handle Bezel Finish Cover
4 | Front Side Door Trim Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
5 | Front Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

6 | Front Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

7 | Front Side Door Trim Panel Retainer (Qty: 9)