For 1990-2009 cars

## Windshield Washer Solvent Container Replacement Acadia and Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
3. Disconnect the washer pump hoses.
4. Drain the washer solvent into a suitable clean container.
5. Disconnect the washer pump electrical connectors.
6. Disconnect the windshield washer level indicator electrical connector.
7. Disconnect the upper neck from the lower portion of the washer solvent container.

1 | Windshield Washer Solvent Container Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Windshield Washer Solvent Container

#### Procedure

1. Remove the container from the front side rail studs.
2. Transfer the washer pumps as needed.
3. Transfer the level indicator as needed.

## Windshield Washer Solvent Container Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the washer pump hoses.
3. Drain the washer solvent into a suitable clean container.
4. Disconnect the washer pump electrical connectors.
5. Disconnect the windshield washer level indicator electrical connector.
6. Disconnect the upper neck from the lower portion of the washer solvent container.

1 | Windshield Washer Solvent Container Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Windshield Washer Solvent Container

#### Procedure

1. Remove the container from the front side rail studs.
2. Transfer the washer pumps as needed.
3. Transfer the level indicator as needed.