For 1990-2009 cars

## Windshield Wiper Blade Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the wiper arm to the full up position in order to release the wiper blade from the wiper arm.

1 | Windshield Wiper Blade Assembly (Qty: 2)

#### Procedure

1. Press the square tab inward at the tip of the wiper arm to release the blade.
2. Slide the blade assembly from the wiper arm.
3. Discard the blade if the rubber element appears worn, or does not wipe the windshield clean.

## Windshield Wiper Blade Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the wiper arm to the full up position in order to release the wiper blade from the wiper arm.

1 | Windshield Wiper Blade Assembly (Qty: 2)

#### Procedure

1. Press the square tab inward at the tip of the wiper arm to release the blade.
2. Slide the blade assembly from the wiper arm.
3. Discard the blade if the rubber element appears worn, or does not wipe the windshield clean.

## Windshield Wiper Blade Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the wiper arm to the full up position, service up.

1 | Windshield Washer Blade Assembly

#### Procedure

1. Squeeze the tabs at the tip of the wiper arm to release the blade.
2. Rotate the blade upward and slide the blade assembly from the wiper arm.
3. Discard the blade if the rubber element appears worn, or does not wipe the windshield clean.

## Windshield Wiper Blade Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the wiper arm to the full up position in order to release the wiper blade from the wiper arm.

1 | Windshield Wiper Blade Assembly (Qty: 2)

#### Procedure

1. Press the square tab inward at the tip of the wiper arm to release the blade.
2. Tilt and slide the blade assembly from the wiper arm.
3. Discard the blade if the rubber element appears worn, or does not wipe the windshield clean. Refer to Wiper Blade Element Check.