For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove Liftgate Door Sill Plate. Refer to Liftgate Door Sill Plate Replacement

1 | Liftgate Lock Striker Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Liftgate Lock Striker

#### Procedure

Mark the location of the striker with a grease pencil to ensure proper alignment during installation.