For 1990-2009 cars

## Rear Seat Recliner Outer Finish Cover Replacement - Outboard with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Outer Finish Cover

#### Procedure

1. Move the seat forward to the Smart Slide® E-Z entry position.
2. Remove the rear seat recliner outer finish cover by pulling outward to disengage the retainers.

## Rear Seat Recliner Outer Finish Cover Replacement - Outboard with 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Outer Finish Cover

#### Procedure

1. Move the seat forward to the Smart Slide® E-Z entry position.
2. To remove the finish cover, release the two tabs that attach to the rear filler panel first. Then pull outward to release the push in retainer and two retainer clips.