For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Fluid Drain Plug Caution: Refer to Fastener Caution in the Preface section. Tip Place a drain pan capable of containing more than 5 quarts of fluid under the transmission before removing the plug to drain the fluid. Tighten
12 N·m (106 lb in)

2 | Fluid Level Indicator Tip

• | Transmission will require approximately 5 quarts of fluid.

• | Fill the transmission with fluid. Refer to Transmission Fluid Check.