For 1990-2009 cars

## Audio System Transceiver Module Replacement U42

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the video display assembly. Refer to Video Display Replacement .

1 | Roof Console Assembly Refer to Roof Rear Console Replacement .
2 | Audio System Transceiver Module Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Use a flat bladed tool to release the tabs that secure the module to the roof console on each side of the module.
3. Slide forward and up to release from the roof console.

## Audio System Transceiver Module Replacement U42/C3U

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the video display assembly. Refer to Video Display Replacement.

1 | Roof Console Assembly Refer to Roof Rear Console Replacement.
2 | Audio System Transceiver Module Mounting Bracket Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Audio System Transceiver Module Mounting Bracket
4 | Audio System Transceiver Module Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Use a flat-bladed tool to release the tabs that secure the module to the bracket on each side of the module.
3. Slide out to release the module from the bracket.