For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Frame Mounting Bolt | 100 N·m plus 90 degrees | 74 lb ft plus 90 degrees
Front Frame Reinforcement Mounting Bolt | 50 N·m | 37 lb ft
Power Steering Fluid Cooler Nut | 30 N·m | 22 lb in
Power Steering Gear Inlet and Outlet Pipe Clip Bolt | 9 N·m | 80 lb in
Power Steering Gear Inlet Hose Bracket Nut | 8 N·m | 71 lb in
Power Steering Gear Inlet Hose Fitting | 27 N·m | 20 lb ft
Power Steering Gear Inlet Hose Retaining Plate Bolt | 12 N·m | 106 lb in
Power Steering Gear Outlet Hose Bracket Bolt | 8 N·m | 71 lb in
Power Steering Gear Outlet Hose Bracket Nut | 8 N·m | 71 lb in
Power Steering Pump Bolt | 50 N·m | 37 lb ft
Rear Front Frame Mounting Bolt | 100 N·m | 74 lb ft
Remote Power Steering Fluid Reservoir Bolt | 9 N·m | 80 lb in
Remote Power Steering Fluid Reservoir Bracket Bolt | 9 N·m | 80 lb in
Steering Gear Bolt (at the right side) | 100 N·m | 74 lb ft
Steering Gear Nut (at the left side) | 75 N·m | 55 lb ft
Steering Gear Heat Shield Bolt | 7 N·m | 62 lb in
Steering Gear Valve Solenoid Bolt | 8 N·m | 71 lb in
Steering Linkage Inner Tie Rod Housing | 100 N·m | 74 lb ft
Steering Linkage Inner Tie Rod Nut | 75 N·m | 55 lb ft
Steering Linkage Outer Tie Rod Nut

- First Pass

30 N·m

22 lb ft

- Second Pass

Plus 120 degrees

Plus 120 degrees