For 1990-2009 cars

## Front Bumper Lower Fascia Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Lower Fascia Tab

#### Procedure

1. Remove the screws from the ends of the upper and lower fascia.
2. Carefully push a small nylon wedge between the fascia and the lower fascia. Insert a small flat-bladed tool into the fascia slot and depress the tabs one at a time and pull on the fascia at the same time to gradually remove the lower fascia from the fascia.

2 | Front Bumper Lower Fascia

## Front Bumper Lower Fascia Replacement Outlook

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.

1 | Front Bumper Lower Fascia Tab

#### Procedure

1. Remove the screws from the ends of the upper and lower fascia.
2. Carefully push a small nylon wedge between the fascia and the lower fascia. Insert a small flat-bladed tool into the fascia slot and depress the tabs one at a time and pull on the fascia at the same time to gradually remove the lower fascia from the fascia.

2 | Front Bumper Lower Fascia