For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove left front floor console extension panel.
2. Remove Floor Outlet Air Duct. Refer to Floor Air Outlet Duct Replacement - Left Side.
3. Reposition any wiring harness to access heater core cover.

1 | Heater Core Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Heater Core Cover