For 1990-2009 cars

## Instrument Panel Cluster Trim Plate Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left instrument panel trim panel. Refer to Instrument Panel Trim Panel Replacement - Left Side.

1 | Instrument Panel Cluster Trim Plate Assembly
2 | Retainer Clips (Qty: 6)

## Instrument Panel Cluster Trim Plate Replacement Acadia

Callout | Component Name
--- | ---
1 | Instrument Panel Cluster Trim Plate Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Trim Plate Assembly
3 | Retainer Clip (Qty: 4)

## Instrument Panel Cluster Trim Plate Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left instrument panel trim plate. Refer to Instrument Panel Trim Plate Replacement - Left Side.
2. Disengage the instrument panel accessory trim plate from the instrument panel assembly. Do not remove completely from vehicle. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Instrument Panel Cluster Trim Plate Assembly

#### Procedure

Use a flat-bladed plastic trim tool in order to release the clips retaining the cluster trim plate to the instrument panel assembly.