For 1990-2009 cars

## Front Bumper Fascia Molding Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the bumper fascia. Refer to Front Bumper Fascia Replacement .

1 | Front Bumper Fascia Molding

#### Procedure

1. Remove the screws from each side before removing the molding.
2. Transfer any necessary parts.

## Front Bumper Fascia Molding Replacement Enclave

Callout | Component Name
--- | ---
1 | Front Bumper Fascia Molding Tip Gently pull on the molding.