For 1990-2009 cars

## Front Bumper Fascia Upper Support Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the hood primary and secondary latch. Refer to Hood Primary and Secondary Latch Replacement.
3. Remove the radiator upper support mounting bolts and position rearward.

1 | Front Bumper Fascia Support Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Bumper Fascia Support

## Front Bumper Fascia Upper Support Replacement Outlook, Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the hood latch support. Refer to Hood Latch Support Replacement.
3. Remove the radiator upper support mounting bolts and position rearward.

1 | Front Bumper Fascia Support Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Bumper Fascia Support