For 1990-2009 cars

## Backup Lamp Applique Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Remove the back up lamp assembly bulb socket from the back up lamp applique.

1 | Back Up Lamp Applique Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Back Up Lamp Clamp (Qty: 2) Tip Remove the clamps from the lamp assembly in order to remove the lamp from the liftgate.
3 | Back Up Lamp Applique Assembly

## Backup Lamp Applique Replacement Acadia

### Removal Procedure

1. Remove the liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Disconnect the backup lamp and running lamp electrical connectors.
3. Remove the screw (1) securing the lamp assembly bracket (2) to the rear auxiliary back up lamp assembly.
4. Remove the bracket.
5. Remove the auxiliary back up lamp assembly nuts (1).
6. Disconnect the backup lamp bulb socket (2) and bulb (3).
7. Pull the backup lamp assembly (2) from the outer liftgate filler panel.
8. Remove the lamp assembly gasket (1).

### Installation Procedure

1. Position the backup lamp gasket (1) to the auxiliary back up lamp assembly (2).
2. Insert the backup lamp assembly into the holes in the outer liftgate filler panel.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the nuts (1).

Tighten
5 N·m (44 lb in).

4. Install the back up lamp bulb (3) into the bulb socket (2).
5. Install the bulb assembly into the lamp.
6. Position the auxiliary backup lamp bracket (2) onto the backup lamp assembly.
7. Install the screw (1).

Tighten
2 N·m(18 lb in).

8. Connect the backup lamp and running lamp electrical connectors.
9. Install the interior liftgate trim panel. Refer to Liftgate Trim Panel Replacement.

## Backup Lamp Applique Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Disconnect the electrical connector at the back up lamp applique.

1 | Back Up Lamp Applique Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Integral Clips (Qty: 2) Tip Release the clips securing the lamp assembly to the liftgate outer filler panel and push outward.
3 | Back Up Lamp Applique Assembly
4 | Back Up Lamp Applique Assembly Gasket Tip Ensure the gasket is in place prior to the back up lamp applique installation.