For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear coil spring and related parts. Refer to Rear Spring, Insulator, and Jounce Bumper Replacement.

1 | Rear Lower Control Arm Nut (Qty: 2)
2 | Rear Lower Control Arm Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten

• | Tighten the front control nut to 110 N·m (81 lb ft) plus 45 degrees

• | Tighten the rear control nut to 120 N·m (89 lb ft) plus 60 degrees

3 | Rear Lower Control Arm