For 1990-2009 cars

### Removal Procedure

1. Apply several layers of masking tape (1) to the mirror lower housing edge (2) to protect the finish.
2. Remove the mirror lens as follows:

2.1. | Push the top center of the mirror inward.

2.2. | Place one hand behind the mirror housing (2) holding the mirror lens (1) in place.

2.3. | Use a suitable rigid plastic tool (3) 3.81 cm (1.5 in) wide. Insert the rigid plastic tool (3) 3 cm (1.5 in) between the mirror lower housing edge (4) and the lower edge of the mirror lens (5).

2.4. | Lift upward on the rigid plastic tool (3) until the mirror lens (1) releases from the motor/actuator ring.

3. Disconnect the electrical connectors from the back of the mirror lens.
4. The motor/actuator ring (1) must stay with the motor/actuator, Not with the mirror lens (2).

Note: When removing the motor/actuator ring, use care Not to damage the mirror lens.

5. If the mirror motor/actuator ring (1) stays attached to mirror lens (3), the motor/actuator ring (1) MUST be removed from the mirror lens.

5.1. | Place the mirror lens face down on a soft cloth.

5.2. | Remove the motor/actuator ring (1), by sliding the ring downward releasing the tabs (2) from the back mirror lens (3).

### Installation Procedure

1. Install the motor/actuator ring (1) to the actuator (2), ensure that the actuator tabs (3) are in line with the motor/actuator ring.
2. Place the motor/actuator ring (1) in the center of the motor/actuator (2).

2.1. | Place mirror lens motor/actuator ring in the center of the motor, press inward until fully seated.

2.2. | Connect the electrical connectors to the mirror lens.

3. Install the mirror lens as follows:

3.1. | Position the mirror lens (1) on the mirror motor/actuator ring lower retaining tabs (2).

3.2. | Place your hand in the back of the mirror housing.

3.3. | Push downward use your hand until the mirror lens (1) locks onto the upper retaining tabs (2).

4. Inspect the mirror lens for proper operation.