For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result. Caution: After cleaning the transmission components, allow to air dry. Do not use cloth or paper towels in order to dry any transmission components. Lint from the towels can cause component failure.

Caution: Do not reuse cleaning solvents. Previously used solvents may deposit sediment which may damage the component.

#### Preliminary Procedure

Clean and inspect all valve components and the valve body. The control valve lower body is replaceable only as an assembly.

1 | 3-5 Reverse Clutch Boost Valve Train
2 | Accumulator Feed Limit Valve Train
3 | 4-5-6 Clutch Boost Valve Train
4 | 4-5-6 Clutch Accumulator Piston Assembly
5 | 1-2-3-4 Clutch Boost Valve Train
6 | 1-2-3-4 Clutch Regulator Valve Train
7 | Control Valve Body Locating Pins (Qty: 2) Tip Inspect Valve Body locating pins for proper installed height of 4.25 mm (0.17 in).