For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the sunroof window. Refer to Sunroof Window Replacement .

1 | Sunroof Window Sealing Strip

#### Procedure

1. Carefully remove the sunroof window weatherstrip from the perimeter of the sunroof window.
2. Use a plastic tool in the removal of the weatherstrip from the sunroof retainer. When reinstalling the weatherstrip, spray a 50/50 soap mix on the edge of the retainer to assist in the reinstall.
3. Place the weatherstrip seam in the rear center of the sunroof window .
4. Place the weatherstrip around all four corners before working the weatherstrip into the retainer.
5. Carefully install the sunroof window weatherstrip to the perimeter of the sunroof window, ensuring that the weatherstrip is fully seated.
6. Ensure that the sunroof does not have any air or water leaks. Refer to Sunroof Window Height and Opening Fit Adjustment .