For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Liftgate Latch Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Liftgate Latch Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Calibrate the liftgate. Refer to Liftgate Calibration.
3. Adjust the liftgate if needed. Refer to Liftgate Adjustment.