For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement.
2. Remove the seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Front Seat Recliner Inner Finish Cover Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Front Seat Recliner Inner Finish Cover (Qty: 2)