For 1990-2009 cars

## Rear Seat Head Restraint Guide Replacement with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Head Restraint

#### Procedure

1. Push down on the seat back cover at the base of the head restraint to access the clips on the head restraint guides.
2. Remove the head restraint guide clips to release the head restraint.
3. Slide the head restraint up to remove.

2 | Rear Seat Head Restraint Guide (Qty: 2)

#### Procedure

1. Loosen the rear seat back cover and pad enough to gain access to the head restraint guides from the front of the seat back.
2. Squeeze together the bottom of the head restraint guide and push upward to remove.

## Rear Seat Head Restraint Guide Replacement with 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Head Restraint

#### Procedure

1. Push down on the seat back cover at the base of the head restraint to access the clips on the head restraint guides.
2. Remove the head restraint guide clips to release the head restraint.
3. Slide the head restraint up to remove.

2 | Rear Seat Head Restraint Guide (Qty: 2)

#### Procedure

1. Loosen the rear seat back cover and pad enough to gain access to the head restraint guides from the front of the seat back.
2. Squeeze together the bottom of the head restraint guide and push upward to remove.