For 1990-2009 cars

## Air Conditioning Condenser Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the A/C discharge line at condenser. Refer to Discharge Hose Replacement.
3. Remove the A/C liquid line at condenser. Refer to Liquid Line Replacement.
4. Pinch fastening tabs together at top of condenser and slide upward to remove.

1 | Condenser Assembly Tip Bottom of condenser mounts into holding fixtures at bottom of radiator.

## Air Conditioning Condenser Replacement Acadia, Outlook, Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement
3. Remove the A/C discharge line at condenser. Refer to Discharge Hose Replacement.
4. Remove the A/C liquid line at condenser. Refer to Liquid Line Replacement.
5. Pinch fastening tabs together at top of condenser and slide upward to remove.

1 | Condenser Assembly Tip Bottom of condenser mounts into holding fixtures at bottom of radiator.