For 1990-2009 cars

## Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement Acadia w/RPO UV6

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side .

1 | Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle

#### Procedure

1. Use a flat-bladed plastic trim tool in order to release the upper trim panel from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the upper trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 10)

## Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement Acadia w/o RPO UV6

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side .

1 | Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle

#### Procedure

1. Use a flat-bladed plastic trim tool in order to release the upper trim panel from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the upper trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 10)

## Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side .

1 | Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle

#### Procedures

1. Use a flat bladed plastic trim tool in order to release the upper trim panel from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the upper trim plate, transfer all necessary components.

2 | Retainer Clips (Qty: 11)

## Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side.

1 | Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle

#### Procedure

1. Use a flat-bladed plastic trim tool in order to release the upper trim panel from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the upper trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 10)

## Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield garnish moldings. Refer to Windshield Garnish Molding Replacement - Left Side and Windshield Garnish Molding Replacement - Right Side.

1 | Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle

#### Procedures

1. Use a flat bladed plastic trim tool in order to release the upper trim panel from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the upper trim plate, transfer all necessary components.