For 1990-2009 cars

Table 1: | Electronic Brake Control Module Scan Tool Data Parameters
Table 2: | Electronic Brake Control Module Scan Tool Output Controls

#### Electronic Brake Control Module Scan Tool Data Parameters

Parameter | System State | Expected Value | Definition
--- | --- | --- | ---
Operating Conditions: Ignition ON
ABS Active | -- | No | The scan tool displays Yes or No. Yes is displayed if the ABS system is engaged.
ABS Failed | -- | No | The scan tool displays Yes or No. Yes is displayed if there is an ABS fault.
Battery Voltage Signal | -- | B+ | This displays volts. This is the voltage status of the electronic brake control module (EBCM).
Brake Booster Vacuum | -- | kPa | The scan tool displays the vacuum pressure in the power brake booster.
Brake Fluid Level Status | -- | OK | The scan tool displays OK or Low. This is the state of the brake fluid level.
Brake Pressure Sensor Input | Engine running | 0 Volts at rest | The scan tool displays 0 Volts at rest and 0.1-2 volts with the brake applied.
BPP Signal | -- | Released | The scan tool displays Applied or Released. This is the state of the brake pedal.
Delivered Torque | -- | 0% | The scan tool displays 0-100%. The scan tool displays the duty cycle of the delivered torque PWM signal. The duty cycle of the signal is used to transmit how much engine torque the ECM is delivering. Normal values are between 10 and 90 percent duty cycle.
DRP Active | -- | No | The scan tool displays Yes or No. This is the state of the dynamic rear proportioning (DRP).
DRP Disabled | -- | No | The scan tool displays Yes or No. This is the state of the dynamic rear proportioning (DRP).
Engine Drag Control Failed | -- | No | The scan tool displays Yes or No. The state of the engine drag control depends on the state of traction of the tires and engine RPM.
LF Wheel Speed Sensor | -- | 0 km/h (0 mph) | This displays km/h (mph). This is the current speed of the left front wheel speed sensor.
LF Inlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the left front inlet valve solenoid is commanded on.
LF Outlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the left front outlet valve solenoid is commanded on.
LR Wheel Speed Sensor | -- | OK | The scan tool displays OK or Low. This is the state of the washer fluid level.
LR Inlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the left rear inlet valve solenoid is commanded on.
LR Outlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the left rear outlet valve solenoid is commanded on.
Panic Brake Assist Failed | -- | No | The scan tool displays Yes or No. The state of the panic brake assist depends on the state of traction of the tires and engine RPM.
Pump Motor Command Voltage | -- | Varies | This displays Volts. This is the voltage status of the EBCM pump motor command.
Requested Torque | -- | 0% | The scan tool displays 0-10%. The scan tool displays the duty cycle of the Requested Torque PWM signal. The duty cycle of the signal is used to transmit how much engine torque the EBCM is requested.
RF Inlet Solenoid | -- | Off | The scan tool displays On or Off. On is displayed when the right front inlet valve solenoid is commanded on.
RF Outlet Solenoid | -- | Off | The scan tool displays On or Off. On is displayed when the right front outlet valve solenoid is commanded on.
RF Wheel Speed Sensor | -- | 0 km/h (0 mph) | This displays km/h (mph). This is the current speed of the right front wheel speed sensor.
RR Inlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the right rear inlet valve solenoid is commanded on.
RR Outlet Solenoid Command | -- | Off | The scan tool displays On or Off. On is displayed when the right rear outlet valve solenoid is commanded on.
RR Wheel Speed Sensor | -- | 0 km/h (0 mph) | This displays km/h (mph). This is the current speed of the right front wheel speed sensor.
Steering Wheel Position | -- | Varies | This displays degrees. This is the signal received from the steering angle sensor.
TCS Active | -- | No | The scan tool displays Yes or No. This is the state of the traction control system (TCS).
TCS Failed | -- | No | The scan tool displays Yes or No. This is the state of the traction control system (TCS).
VSES Active | -- | No | The scan tool displays Yes or No. The scan tool displays Yes when VSES is active, and No when VSES is inactive.
VSES Actuator Commanded | -- | Varies | This displays amps. This is the amount of current applied to the VSES actuator.
VSES Actuator Feedback Signal | -- | Varies | This displays amps. This is the amount of current applied to the VSES actuator feedback signal.
VSES Failed | -- | No | The scan tool will display Yes or No depending on the state of the ABS indicator.
Yaw Rate Sensor | -- | Varies | This displays Volts. The voltage varies depending on the angle of the vehicle.

#### Electronic Brake Control Module Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
ABS Motor Test | This is used in order to command the ABS pump motor On or Off.
Automated Bleed | This is used in order to bleed ABS hydraulics. Refer to Antilock Brake System Automated Bleed Procedure.
Brake Press. Sen. Calibration | This is used in order to calibrate the brake pressure sensor.
LF Inlet Valve Solenoid | Commands the solenoid ON and OFF.
LF Outlet Valve Solenoid | Commands the solenoid ON and OFF.
LR Inlet Valve Solenoid | Commands the solenoid ON and OFF.
LR Outlet Valve Solenoid | Commands the solenoid ON and OFF.
RF Inlet Valve Solenoid | Commands the solenoid ON and OFF.
RF Outlet Valve Solenoid | Commands the solenoid ON and OFF.
RR Inlet Valve Solenoid | Commands the solenoid ON and OFF.
RR Outlet Valve Solenoid | Commands the solenoid ON and OFF.
Steering Angle Sensor Centering | This is used to center the steering angle sensor.
VES Test | This is used to test the variable effort steering (VES) actuator.