For 1990-2009 cars

1. Install the NEW intake manifold gasket.
2. Install the intake manifold assembly.
3. Install the intake manifold bolts.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the intake manifold bolts in the sequence shown.
5. Tighten the intake manifold bolts in sequence to 23 N·m (17 lb ft).
6. Tighten the intake manifold bolts a second pass in sequence to 23 N·m (17 lb ft).
7. Install the fuel pump cover (2).
8. Install the fuel pump cover bolt (1) and tighten to 10 N·m (89 lb in).
9. Install the evaporative (EVAP) solenoid.
10. Install the EVAP solenoid bolts and tighten to 10 N·m (89 lb in).
11. Connect the EVAP hose to the upper intake manifold and EVAP solenoid.
12. Connect the positive crankcase ventilation (PCV) tube assembly to the upper intake manifold and the right camshaft cover.
13. Install the brake booster hose to the upper intake manifold.