For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lift and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Fuel Pump Flow Control Module Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip The bolts used are two headed and can be loosened from the module side, then maneuvered out of the slots. Tighten
9 N·m (80 lb in)

2 | Fuel Pump Flow Control Module

#### Procedure

1. Disconnect the electrical connector.
2. If replacing the fuel pump flow control module, program the control module. Refer to Control Module References.