For 1990-2009 cars

## Front and Rear Side Door Lower Weatherstrip Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open both doors on the side the rocker panel weatherstrip will be replaced.

1 | Front and Rear Side Door Lower Weatherstrip Retainer (Qty: 15) Tip With a suitable trim release tool, release the 15 retainers securing the weatherstrip to the front and rear rocker panel molding.
2 | Front and Rear Side Door Lower Weatherstrip Assembly